

|  |
| --- |
| **Instructions for Painting Shark Fins on Concrete Surfaces****Materials:**Stencils – made of thick cardboard traced from previous fins Brushes – small rollers, sponges and regular big and small paint brushesMasking tapePaint, primer and sealer **1st Step:** Trace FinsNew fins – trace fins and apply concrete primerExisting fins – tape fin outline and skip to step 2 **2nd Step:** Apply Base Color Sherwin Williams Satin Porch & Floor EnamelTricorn Black (SW 6258) or Serious Gray (SW 6256) **3rd Step:** Outline FinSherwin Williams Satin Porch & Floor Enamel Extra White or Serious Gray (SW 6256) **4th Step:** Decorate FinPaint athlete’s name, jersey # and other decorationsSherwin Williams Satin Porch & Floor Enamel Extra White, Serious Gray (SW 6256), Blue Click (SW 6952) **5th Step (Optional):** Apply SealerConcrete Sealer Clear Gloss **Notes:*** Power wash or clean well before project begins
* Paint colors on file at Sherwin Williams in Ponte Vedra Beach
* Best to paint when the surface is dry and the concrete is not too hot
* Decorate within the outline of the fin
 |

