

|  |
| --- |
| **Instructions for Painting Shark Fins on Concrete Surfaces**  **Materials:**  Stencils – made of thick cardboard traced from previous fins  Brushes – small rollers, sponges and regular big and small paint brushes  Masking tape  Paint, primer and sealer    **1st Step:** Trace Fins  New fins – trace fins and apply concrete primer  Existing fins – tape fin outline and skip to step 2    **2nd Step:** Apply Base Color  Sherwin Williams Satin Porch & Floor Enamel  Tricorn Black (SW 6258) or Serious Gray (SW 6256)    **3rd Step:** Outline Fin  Sherwin Williams Satin Porch & Floor Enamel  Extra White or Serious Gray (SW 6256)    **4th Step:** Decorate Fin  Paint athlete’s name, jersey # and other decorations  Sherwin Williams Satin Porch & Floor Enamel  Extra White, Serious Gray (SW 6256), Blue Click (SW 6952)    **5th Step (Optional):** Apply Sealer  Concrete Sealer Clear Gloss    **Notes:**   * Power wash or clean well before project begins * Paint colors on file at Sherwin Williams in Ponte Vedra Beach * Best to paint when the surface is dry and the concrete is not too hot * Decorate within the outline of the fin |

